**Dr. Y. S. R. HORTICULTURAL UNIVERSITY**

**VENKATARAMANNAGUDEM – 534 101**

**TENDER DOCUMENT**

**FOR**

**SUPPLY, INSTALLATION & COMMISSIONING OF COMMUNITY RADIO STATION (CRS) AND VIDEO PRODUCTION EQUIPMENT**

**AT**

**Dr.YSRHU-COLLEGE OF HORTICULTURE,**

**ANANTHARAJUPETA, RAILWAY KODURU, 516 105**

**ANNAMAYYA (DIST), ANDHRA PRADESH.**

****

Tender Notice No: No:1/RKVY/Community Radio Station/Dr.YSRHU/COH-Anantharajupeta/

 2025-26

Date of Commencement of : **02.09.2025 at 5.00 PM**

DOWN LOADING OF THE

BID DOCUMENT

Last date for receipt of bids : **15.09.2025 at 5.00 PM**

Dr Y.S.R. Horticultural University

 College of Horticulture, Anantharajupeta,

 Railway Koduru, 516 105

 Annamayya (Dist), Andhra Pradesh.

TIME AND DATE OF

Opening of the bid :**16.09.2025 at 11.00 AM**

ADDRESS FOR COMMUNICATION:

**ASSOCIATE DEAN**

**COLLEGE OF HORTICULTURE, ANANTHARAJUPETA,**

**RAILWAY KODURU, 516 105**

**ANNAMAYYA (DIST), ANDHRA PRADESH**

**Mobile No: 73826 33651**

**email: ad-arpt@drysrhu.edu.in**

The tender document containing terms and conditions for the execution of this project along with specifications and EMD to be paid are appended.

**INVITATION FOR BIDS**

* 1. The location of the site is at **College of Horticulture, Anantharajupeta, Railway koduru, Annamayya (Dst.)** of Andhra Pradesh.
	2. Bids are invited from nationally/internationally reputed manufacturers/their authorized representatives only, for the above said equipment. The authorized representative must attach an authorization letter from the manufacturers along with the tender without which the tender will be rejected (for further reference please refer point 16 in Annexure I (Part-I).
	3. The bidders are also required to furnish their previous experience certificate for the supply of similar equipment.
	4. The supply of equipment must be carried out as per the standard specifications under the supervision of concerned authority of **COH, Anantharajupeta** and duly handing over all warranty certificates for the said equipment.
		+ 1. All bidders must quote equipment; otherwise bid will be summarily rejected.
1. All local taxes to be paid to the government shall be included in the price quoted as F.O.R. destination.
2. Custom duty exemption certificate will be issued in case necessary.

V) The bids should be submitted with in time specified at the office of Associate Dean, **COH,**

 **Anantharajupeta** along with **EMD** as specified here under against each item.

|  |  |  |  |
| --- | --- | --- | --- |
| **S.No** | **Item** | **Qty** | **Location** |
| 1 | Community Radio Station Studio, Acoustic Setup, Transmission System & Accessories (Items 1–42 in Annexure II) | 1 Job | COH, Anantharajupeta |
| 2 | Video Production Equipment (Items 1–9 in Annexure III) | 1 Job | COH, Anantharajupeta |

Bidders must pay the EMD Rs.10,000/- against each of the item in the form of **crossed D.D.** drawn **in favor of The Comptroller, Dr YSRHU,Venkataramannagudem**, Tadepalligudem payable at Union Bank of India (formarly AndhraBank)/ any nationalized bank, Tadepalligudem and processing fee of **Rs.1,000/- (Rupees One thousand only**) through DD **in favor of The Comptroller, Dr YSRHU, Venkataramannagudem**, Tadepalligudem payable at Union Bank of India (formarly AndhraBank)/ any nationalized bank, Tadepalligudem. The processing fee is non-refundable and tender documents without EMD or Processing fee will be rejected.

VI) Specifications given are indicative and the tender is to give a detailed description and specifications for each equipment. The same would be given weightage in finalizing the tender.

VII) The equipment to be supplied by the tenderers should be branded and meet the quality

 standard as per the existing norms.

VIII) The bids invited on two-part basis, the Bidder shall seal the **technical bid** and the **priced bid** in two separate envelops duly **marked as “Technical bid” and “price bid”. Both the envelopes shall then be sealed in one outer envelope.**

All bids must be accompanied by a bid security/Earnest Money Deposit as specified in the tender details and must be delivered to the above office at the date and time indicated above. Bids will be opened in the presence of Bidders' authorized representatives who choose to attend on the specified date and time. In

the event of the date specified for bid receipt and opening being declared as a closed holiday for purchaser’s office, the due date for submission of bids and opening of bids will be the following working day at the appointed time.

IX) Dr.YSR Horticultural University reserves the right to accept any or all tenders either in part or in full or to split the order without assigning any reasons therefore.

X) The specifications and other conditions prescribed in Annexure –II & III of this tender shall also be treated as part of these tender documents for all purposes.

**TERMS OF PAYMENT:**

|  |  |
| --- | --- |
| 1) Against the delivery of complete equipment and installation. | 100% of the project cost. |

XI) This Invitation for Bids is open to all suppliers.

Bidders who have been blacklisted / suspended by the purchaser or sister concerns are ineligible to quote. The quotes of such firms shall be summarily rejected. Prices shall be quoted in Indian Rupees for all offers as FOR –DESTINATION BASED and in case of offers received for supply from foreign countries may comply the offers to a convertible to Indian currency and customs duty as applicable to each item be given separately for parity during evaluation.

**ELIGIBILITY CRITERIA**

1. The preference would be given to manufacturer with experience of having supply of similar equipment’s in reputed Agricultural Universities / State Department of Horticulture / ICAR institutes/private organizations.
2. Certificate from the project client for award of contract and supply of equipment in original or its notarized copy for equipment claimed to be submitted.
3. The company bidding should be in the industry for at least 5 years in the same field. Tenderers should have authorized dealer certificate/ distributor of the OEM/manufacturing certificate (Please attach certificate).
4. Tenderers should have a minimum average annual turnover of **₹ 25 lakhs or above for supply of similar equipment’s. Audited financial statements duly certified by charted accouted** for the last three financial years ending March 31st, 2025 should be submitted.
5. The buyer reserves the right to evaluate the tender on Technical Presentation/ capabilities and is not bound to accept lowest tender / quotations.

**EVALUATION OF BID:**

1. The Technical Bid documents will be opened first and evaluated by the Tender Committee. Financial Bid Documents of only those bidders will be opened who have qualified in Technical Bid.
2. The Competent Authority reserves the right to accept or reject any tender without any reason thereof.
3. Prices to be quoted on FOR basis including all taxes including GST/freight/ installation/commissioning/trial/training charges etc. in Indian rupees.
4. It is necessary to submit all the relevant documents like Processing fee, EMD Rs. 10,000/-, Income tax return files for last 3 years, GST/Sales Tax Registration, Authorized dealer of a reputed company or proof of being an authorized distributor of the OEM, along with technical bid.
5. Tenderer should submit the copies of Purchase Orders in support of their genuineness in supplying of equipment’s in reputed Universities / Colleges / Departments / Institutes/private organizations. The tenderer should submit users list for the last 5 years.
6. It is necessary to submit all the relevant documents like Pan Card, ISO Certification, GST/Sales Tax Registration, Authorized dealer of a reputed company or proof of being an authorized distributor of the OEM, Certificate of Incorporation / Partnership Deed, In-voice, Make and model, warranty and installation details along with financial bid.

**DISQUALIFICATION:**

The EOI may, at its own sole discretion, at any time during the EOI process, disqualify any Interested party from the EOI process if:

1. the response to the tender is submitted after the dead line for submission.
2. the Interested Entity has made misleading or false representation in the forms, statements, attachments submitted in proof of eligibility.
3. the tender is not accompanied by required documentation.
4. the Interested Entity failed to provide clarifications related thereto, when sought.

The Dr.YSRHU reserves the right to verify the claims made by the Bidder and to carry out the capacity assessment of the bidder and the Dr. YSRHU decision shall be final in this regard.

**ANNEXURE – I (PART I)**

**TECHNICAL BID: filling up of Proforma**

 The technical bid shall accompany with the enclosures for components as per proforma prescribed and is attached with the document along with the details as under:

|  |  |  |
| --- | --- | --- |
| **S. No.** | **Intervention/Component** | **Annexure****(With page nos.)** |
| 1 | Company Profile |  |
| 2 | Past Experience of manufacturer with certificates/ work order/ completion etc. |  |
| 3 | No. of years of experience in this field |  |
| 4 | Past experience in supply of equipment |  |
| 5 | Experience of Engineers/ technician and the capacity for service with service center |  |
| 6 | Financial Strength of the Firm |  |
| 7 | Office details |  |
| 8 | GST registration certificate |  |
| 9 | Any others as specified in the general bid document |  |

**General Terms & Conditions:**

1. Technical quote / bid and price quote / bid, should be submitted separately.
2. A compliance statement in detail for each individual technical parameters / component of each instrument including warranty etc. as given in each instrument should be prepared by the vendor in the Technical Bid.
3. Each firm should submit separately technical specifications as at serial no.2 in one single envelope – technical quote. However, the price bids for equipment quoted with the offer should be submitted separately for equipment wise.
4. Validity of quotations/tenders should be at least 3 months from last date of receipt of quotations/tenders.
5. Product brochures should be enclosed for equipment.
6. Make and Model should be mentioned clearly.
7. Name of the customer/s with telephone, e-mail ID should be given, for each instrument, separately.
8. The service network team/persons with contact numbers, mailing address, e-mails preferably in AP should be given for each instrument separately.
9. If the instrument is imported, the supplier should take all responsibilities for clearing, duties, delivery etc.,
10. Installation should be at free of cost.
11. Training to be provided at free of cost.
12. All the supplies should be through authorized dealer/distributor in AP (Authorized dealer / distributor certificate should be enclosed along with quotations/tenders).
13. All quotations / tenders for each instrument should have compliance report as per the specifications mentioned point wise.
14. The instruments should be delivered at **COH, Anantharajupeta** at free of cost or the price quoted should include the delivery and handling charges, if any. No additional charges will be paid towards delivery and installation. Further, 5% GST has to be provided as university provides the DSIR certificate.
15. All instruments should be supplied along with hard copies of operating manual and soft copies in CD/DVD / flash drive/software’s, wherever required.
16. For all imported equipment’s, the supplier holds the responsibility for clearance, and delivery to the destination at **COH, Anantharajupeta**. Dr. YSRHU will issue customs exemption certificate as applicable and as available at the time of clearance.
17. The quotations/tenders should be submitted in a sealed cover super scribing “**Quotation/ Tender (TECHNICAL BID/ PRICE BID) for supply of\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (S.No: ) for COH, Anantharajupeta Andhra Pradesh**”.

The Dr. Y.S.R.H.U reserves the right to verify the claims made by the Bidder and to carry out the capacity assessment of the bidder and Dr Y.S.R.H.U decision shall be final in this regard.

**Annexure– I (Part–II)**

**“DECLARATIONOF THE BIDDER”**

1. That I/We am/are the authorized nominee (s) of the firm hereby submit tender to College of Horticulture, Anantharajupeta. The copy of the power of Attorney is attached here with.
2. I am to state that the information provided in the tender form is true and correct
3. I/We may be punished as per law for any wrong information, misleading facts provided in the tender form besides rejection of my/our tender.
4. In case of any dispute, the Jurisdiction will be as applicable to Dr YSRHU only.
5. I/We have carefully read all the general and specific terms and conditions of the tender and I solemnly declare that the same are acceptable to me/us and binding on me/us.

Place : Signature of Bidder :

Date :

Name of Bidder :

Capacity in which signed :

Full address of the Bidder : With seal & stamp :

(Attach Identity card Xerox)

Phone No. :

Mobile No. :

# **ANNEXURE – II**

### TECHNICAL SPECIFICATIONS FOR COMMUNITY RADIO STATION (CRS) EQUIPMENT

The bidder must supply, install, and commission the following equipment **as a complete lot**. The specifications provided below are **minimum requirements**. Higher or equivalent configurations may also be considered, subject to documentary proof and compliance statement.

**Room Dimensions:** 12.15x8.95x2.8 Meters

|  |  |  |  |
| --- | --- | --- | --- |
| **S.No.** | **Item Name** | **Quantity** | **Specifications** |
|  | **Partition wall**  | 1 | 200 mm double-skin partition with GI framework, cavity filled with 75–100 mm mineral wool (48–64 kg/m³, IS 8183 compliant), finished both sides with double 12.5 mm fire-rated acoustic gypsum boards, all joints sealed with acoustic sealant. |
|  | **Closing of existing window opeing (size 5.3x5.10 ft) with brick masonry** | 1 | Providing and constructing solid brick masonry inn cement mortar (1:4), plastered on both sides with cement mortar (1:3), finished smooth, matchning existing wall thickness, including curing, scaffolding, and complete finishing as ditected |
|  |  **Acoustic wall panelling, type-I for low frequency sound absorption** | 34 meter2 | Low-frequency absorption panels up to 1.2 m height, fabricated with 4 mm veneer + 6 mm marine ply on aluminum framework, with air cavity up to 15 cm from floor. Finished with melamine polish. The rate includes loading, unloading, lead etc.  |
|  | **Acoustic wall panelling, type-II for mid/high frequency sound absorption** | 110 meter2 | Mid/high frequency panels with 2"x2" aluminum frame, 12 mm ply backing, 50 mm thick 40 kg/m³ density rockwool infill, fabric-finished surface with wooden beading + skirting. |
|  | **Acoustic False Ceiling** | 74 meter2 | Supply and installation of Saint Gobain acoustic ceiling tiles with a minimum NRC (Noise Reduction Coefficient) of 0.90, tile size 600mm x 600mm x 15mm, square edge, installed on a G.I. exposed T-grid suspension system with necessary hangers, channels, and fixtures as per manufacturer’s recommendations. The tiles shall be fire-resistant, sag-resistant, and suitable for studio-grade sound absorption. Installation must ensure a level, clean finish as per acoustic consultant's approval.  |
|  | **PVC Flooring** | 74 meter2 | SITC of 2mm thick homogeneous PVC roll flooring, anti-skid, fire-retardant, water-resistant, factory-laminated finish, suitable for acoustic studio application. |
|  | **Acoustic Door & Chowkhat** | 3 | Studio-grade double-leaf soundproof door with solid core, acoustic seals on all sides, minimum STC 50 rating, factory-finished with heavy-duty hinges. |
|  | **Normal Door & Chowkhat** | 2 | Wooden, standard quality, customized |
|  | **Hydraulic Door Closer** | 3 | Heavy-duty ISI certified hydraulic door closer, adjustable closing speed. |
|  | **Observation Window** | 2 | Acoustically treated 4'x3' window,  |
|  | **On-Air Studio Table** | 1 | Customized ergonomic studio desk, laminated MDF/plywood, cable management channels, rounded edges, vibration-free design. |
|  | **Production Studio Table** | 1 | Customized workstation with laminated MDF/ply top, concealed wiring channels, vibration damping. |
|  | **Discussion Table** | 1 | Round/rectangular table with solid ply/MDF top, melamine polish, cable slots for microphones. |
|  | **Control room table** | 1 | Customized console-type desk, rack space for equipment, MDF laminated top, cable management ducts. |
|  | **Electrical Wiring & LED** | 1 job | Complete electrical wiring, cabling, LED fitting  |
|  | **Conduit & Piping** | 1 job | ISI mark rigid PVC/metal piping for cable routing |
|  | **Earthing System** | 3 | Earthing for studio/transmitter, ISI standard |
|  | **Electrical Panel** | 1 job | Distribution panel (MCB, TPN & wiring) |
|  | **UPS Distribution Cabling & Sockets** | 1 Job | Supply and installation of UPS distribution cabling with ISI-mark copper wires, conduits, MCB protection, and dedicated color-coded sockets (red for UPS, black for raw power) for all studio and workstation equipment, including testing and commissioning. |
|  | **50 W FM (CRS) Transmitter** | 2 | 50 W FM (CRS) Transmitter |
|  | **FM Transmitting Antenna** | 1 | SITC of VHF, wide band, vertically polarized 2 bays, 3dB, omni directional, folded dipole anrtena with N connectors |
|  | **RF Cable** | 1 | 7/8" foam-filled coaxial cable with N connectors, insertion loss ≤0.5 dB/100m. |
|  | **Transmission Rack** | 1 | 19” standard rack, 16U height, 600 mm depth, ventilated, powder-coated, cable manager, earthing kit. |
|  | **Transmission Tower** | 1 | Self-supported 100 ft tower with lightning arrestor |
|  | **Analog Audio Mixer (10-ch)** | 1 | Must include 4 mic/line combo inputs with D-PRE preamps, built-in 24 SPX digital effects, USB 2-in/2-out audio interface (24-bit/192kHz), +48V phantom power, and 1-knob compressors on CH 1–2. |
|  | **Studio Headphones** | 3 | * Closed-back, over-ear wired headphones with lightweight (215 g) design and 3 m cable.
* Frequency response: **21 Hz – 18 kHz**, Impedance: **24 Ω**, Sensitivity: ~**108 dB SPL**.
* 30 mm dynamic drivers, THD < **0.7%**, good passive noise isolation.
* Comes with 3.5 mm plug + 6.3 mm adapter, ideal for studio monitoring and casual listening.
 |
|  | **Audio Distribution Amplifier** | 1 | Ultra-flexible **8-channel splitter/mixer** that can be used as a 2-in/8-out, 8-in/2-out, or 6-in/6-out audio distribution amplifier, wide frequency response **10 Hz – 40 kHz**, low noise with high headroom, balanced XLR and TRS connectors. |
|  | **Equipment Hosting Accessories** | 1 | Mounting kits and stands |
|  | **Installation Material (Audio)** | 1 | Cables, connectors (Installation Materials (Audio) – High-quality shielded audio cables (XLR, TRS, EP) with low noise and durable insulation. Gold-plated connectors/adapters for reliable signal transmission. SDI/HDMI cables supporting Full HD/4K video with strong shielding. All materials should meet broadcast/studio grade standards for long-term use.) |
|  | **16-Ch Audio Mixer (AV)** | 1 | Must include 10 mic/line combo inputs with D-PRE preamps, built-in 24 SPX digital effects, 1-knob compressors on 8 channels, and USB 2-in/2-out interface (24-bit/192kHz). |
|  | **AV Studio Monitor Pair, 50 W** | 1 | Compact **4" powered studio monitors**, delivering **50 W** of clear, balanced sound with JBL’s professional tuning, frequency response approx. **77 Hz – 20 kHz**, front-panel volume control, Bluetooth input, TRS/RCA connectivity. |
|  | **Condenser Mic**  | 5 | Small-diaphragm cardioid condenser type with frequency response 40 Hz – 20 kHz and sensitivity around 15 mV/Pa. Operates on 48V phantom power, with low self-noise (~16 dB-A). Rugged metal body with balanced XLR output, suitable for studio recording and instruments. |
|  | **Dynamic Mic (AV)** | 1 | Cardioid dynamic vocal microphone with tailored frequency response for clear voice reproduction. Frequency response approx. 50 Hz – 16 kHz, sensitivity around –55 dBV/Pa. Rugged design with on/off switch, balanced XLR output, suitable for live sound and AV applications. |
|  | **Table Mic Stand (AV)** | 6 | Compact and sturdy desktop stand with adjustable gooseneck for flexible mic positioning. Heavy weighted base for stability and vibration reduction. Standard 5/8" mic thread, suitable for AV and studio use. |
|  | **3 KVA Online UPS** | 1 | Double conversion technology with IGBT rectifier, unity power factor, and wide input voltage range. Provides pure sine wave output with static bypass, LCD display for monitoring, and intelligent battery management for reliable backup. |
|  | **SMF Batteries** | 6 | Sealed Maintenance Free (VRLA) battery with 12 Volt nominal voltage and 65 Ah capacity. Uses AGM (Absorbent Glass Mat) technology for high reliability, spill-proof design, and longer service life. Suitable for UPS, telecom, and power backup applications. |
|  | **HP Workstation** | 3 | Equipped with an Intel Core i7 processor, 16 GB RAM, dual storage (240 GB SSD + 1 TB HDD), 19.5-inch TFT display, Windows OS preinstalled, and a full-tower desktop chassis. |
|  | **Internet Radio Package** | 1 | A rackmount 10-band audio processor offering dual independent processing paths—one for on-air broadcast and one for internet streaming—with built-in AAC/AAC+ encoder (Icecast/CDN compatible), analog (XLR) and optional AES digital I/O, Ethernet remote control via SoundMax Manager, and universal 105–260 V AC power supply. |
|  | **Phone in equipment** | 1 | professional digital telephone hybrid with 16-bit DSP providing >50 dB separation between caller and talent. It has balanced XLR mic/line input, XLR and 3.5 mm stereo outputs, headphone jack, and RJ-11 phone line/handset connections. Features include auto-answer/disconnect, send/receive level controls, and optional remote control via RJ-45 port. Powered by universal 100–240 V AC adapter.  |
|  | **Split air conditioners, 2 ton** | 3 | 2.0 Ton, inverter type, 4-star energy rating, copper condenser coil, low-noise indoor unit (<40 dB), remote control, 5 yr compressor warranty. |
|  | **Miscellaneous Works, Testing & Commissioning**  | **1 Job** | This shall include final finishing, painting touch-ups, labelling, cable dressing, AC supports, stabilizers, installation & commissioning of all equipment, software setup, training of staff, and any minor works not specifically mentioned but essential for successful functioning of the studio. |
|  | **Transportation Charges** | 1 job | Delivery to site with loading/unloading, proper packing. |

**Note:**

* All equipment must be **brand new, genuine, and factory-sealed**.
* Compliance sheet (point-by-point against each item) must be enclosed.
* Vendors must provide **OEM authorization** for transmitters, consoles, processors, and automation software.

# **ANNEXURE – III**

### TECHNICAL SPECIFICATIONS FOR VIDEO PRODUCTION EQUIPMENT

The bidder must supply, install, and commission the following equipment. All items must be **brand new, factory sealed, and covered under standard OEM warranty.**

**Video Production Equipment**

|  |  |  |  |
| --- | --- | --- | --- |
| **S.****No.** | **Item Name** | **Quantity** | **Specifications** |
|  | Dynamic Microphones (Studio) | 1 | Cardioid dynamic microphone tailored for clear vocal reproduction with frequency response 50 Hz–16 kHz. Rugged design with on/off switch, includes stand adapter and zipper pouch. Supplied without cable (LC version). |
|  | 4K Professional Camcorder  | 1 | Compact professional camcorder with 1.0-type MOS sensor and UHD 4K recording up to 60p. Features 24x optical zoom lens, dual SD card slots, built-in Wi-Fi/NDI streaming, and professional XLR audio inputs. |
|  | Tripod for Camera | 1 | Professional camera tripod with aluminum build, load capacity up to 7–8 kg, and maximum height around 150–170 cm. Quick-release plate with secure locking system for fast mounting. Lightweight, foldable design for portability with stable three-section legs. |
|  | Chroma Stand (10x12')  | 1 | Chroma support stand, size 10x12 ft, with durable steel frame and adjustable height. Designed for holding chroma/green screen backdrops securely in studios.Stable base structure with easy assembly and portability. |
|  | LED Lights (1x1) with Stand | 3 | LED panel light (1x1 ft) with adjustable brightness and color temperature (bi-color 3200K–5600K). High CRI for accurate color rendering, flicker-free output suitable for video recording. Comes with sturdy height-adjustable stand for flexible positioning. |
|  | Teleprompter System | 1 | Teleprompter system with dual display screens and high-quality beam-splitter mirror. Includes user-friendly teleprompter software with remote operation support. Compatible with professional cameras, ensuring clear visibility for presenters. |
|  | Apple Workstation | 1 | Workstation with Apple Silicon M1 chip, 8 GB unified memory and 512 GB SSD storage.Additional 4 TB HDD for extended storage capacity.Retina display with Magic Keyboard and Magic Mouse included for seamless workflow. |
|  | AV Installation Kit (Audio cables, Microphone cables, Connectors/adapters, SDI cables, HDMI cables) | 1 | High-quality professional audio and microphone cables with balanced shielding for noise-free transmission.Durable connectors/adapters (XLR, TRS, EP, RCA) with secure locking for reliable signal flow.SDI cables supporting 3G/6G/12G signals for long-distance professional video transmission.HDMI cables supporting Full HD/4K resolution with gold-plated connectors for stable performance. |
|  | AV Capture Device | 1 | AV capture device with SDI input to HDMI output conversion, supporting 3G-SDI signals.Compact micro design for easy integration in studio and field setups. Delivers real-time, low-latency video output with high-quality signal processing. |

**ANNEXURE – IV**

**(General Conditions)**

### Submission of Tender and Deposit of earnest money

1. Quoted rate should be written legibly in ink or type written. No alterations should be made to any of the terms and conditions of the tenders by scoring out, altering or overwriting; similarly, no alterations are permitted in the rates quoted by them. No alterations will be allowed after this Office receives the tender. Ambiguity must be avoided in filling the tenders. However, any corrections etc., made will have to be duly attested with dated signatures and official seal. The tenders not complying with these conditions will be rejected summarily.
2. The tenders not conforming to the prescribed terms and conditions of the Horticultural University or conditional Tenders or Tenders which cannot adhere to the prescribed time schedule are liable for rejection.

#### Validity of rates and other Conditions

1. The defect liability period for the Equipments and erection of screen house shall be given for 12 months or more from the date of installation. In the event of any correction or defects or replacement of defective material done during this period, it should be corrected/ replaced at the cost of the bidder/ agency.
2. Bids shall remain valid for a period of 90 days from the date of opening of the bid prescribed. In exceptional circumstances, the University may solicit the bidder’s consent for an extension of the period of validity. The request and response shall be made in writing / cable / telex / fax / e-mail.
3. The validity of the tender will extend for a period of three months from the date of placing the initial order and it shall be open to the Dr.YSRHU to place the orders with the suppliers on the same rates, terms and conditions for any additional quantities likely to be recurred during that period.
4. The bidders shall submit the technical bid and price bid in separate covers and kept in a single cover.
5. The inner and outer envelops shall bear the following address:

**THE ASSOCIATE DEAN**

**COLLEGE OF HORTICULTURE-**

**ANANTHARAJUPETA, RAILWAY KODUR -516105**

**ANNAMAYYA (DIST), ANDHRA PRADESH.**

1. The inner envelopes should also contain the name and address of the bidder.
2. Telex, cable, e-mail or facsimile bids will be rejected.
3. Bidding Documents must be received by the University at the address specified not later than the time and date specified in the invitation (Notification) for bids.
4. In theevent of the date specified being declared as a holiday for the University, the bids will be received up to the appointed time on the next working day.
5. The Bidder’s representatives who are present shall sign in the register evidencing their attendance.
6. During evaluation of bids subsequent to opening, the University may at its discretion, to ask the bidder for clarification of its bid. The request for clarification and the response shall be in writing and no-change in the bid will be entertained.
7. The evaluation of the bid will take into account, the past experience in addition to the bid price. Such price should include all duties and taxes to be paid or payable on components of works.
8. The bidder may present power point presentation to Committee on the following.
9. Equipment related and their working performance
10. Operation and maintenance

**Acceptance of tenders**

1. Price bids will be opened after completion of power point presentation in the presence of such tenderers who are qualified in technical bid as may be present. A decision with regard to acceptance of tender will be taken as soon as possible.
2. The successful tenderer (s) will be intimated by letter (s) or other means of communication and the tenderer (s) so informed shall be bound from the time of transmission of such acceptance by the University. Formal acceptance of the tender (s) will be forwarded to successful tenderer (s) in due course but it will serve merely as a confirmation of the initial information and shall not affect the time from which the offer is/are is bound by the contract(s).
3. The University is not bound to accept the lowest tender. Any or all the quotations may be rejected without assigning any reasons. It reserves the right of acceptance in whole or part of the offer made. The decision of the Dr.YSR Horticultural University in the matter shall be final and binding on the tenderers.
4. 2% of income tax will be deducted from each item of the approved tender item.

**TENDER EVALUATION**

The evaluation and comparison of the bids shall be done for the technical as well as financial aspects.

**a) Technical Bid Evaluation:**

While power point presentation or the examination of the documents submitted by the tenderer, the committee shall have the right to verify the claims of experience made by the bidders. Based on the bid evaluation, only technically qualified bidders shall be short listed. After thorough evaluation of the technical bid by the committee, the financial bid of only technically qualified Bidders shall be opened in due course.

**b) Financial Bid Evaluation:**

 The total cost of the project (landed cost) quoted by the bidder would be considered for financial bid evaluation.

**Committee:**

1. The committee shall do the above evaluation. The committee shall determine the approach and methodologies for the issues, which may arise during the above, referred evaluation process and their decision is final. The decision of the committee to reject or accept shall be final and binding on all the bidders.
2. The successful bidder shall be responsible for the maintenance of the equipment for a period of ONE YEAR from the date of installation. The bidder shall deploy at least one experienced person from time to time for advising any doubts regarding operation and maintenance besides troubleshooting whenever required.

#### Other contractual obligations

1. The contract shall not be deferred/ modified except by written consent by both Dr. YSRHU and the Bidder.
2. The Bidder shall not sublet or delegate this contract or part thereof without the written consent of the Horticultural University.
3. No undertaking or commitment given by or made by any officer of the University verbally or in writing does not have any validity unless it is signed again by the authority competent who concluded an agreement earlier.

#### Consequence of non-supply and damages

1. All risks of loss, damage or depreciation to the equipment/ material there off shall be upon the supplier until the material is delivered at the addresses specified and in accordance with the provision of the contract. Till the material is received at the respective destination indicated by the university, the property continues to be at the risk of the Bidder.The mere fact that the material is delivered to transporter is no defense to the Bidder and the Bidder will be squarely held responsible for any delayed receipt of the material by the University or for loss or damage of any kind to the material in transit.
2. Assuming that the bidder fails to deliver any or all the material covered by the contract, the Horticultural University reserves the right in addition to other legal remedies, to cancel the contract or any portion thereof and hold the Bidder liable for all damages sustained by the university by virtue of the Bidder failing to perform the contract and consequent cancellation of the contract.
3. The time allowed for delivery of goods shall be deemed to be the essence of the contract. The University also reserves the right to cancel the purchase order in case supplies are delayed beyond the scheduled date of delivery and to make such arrangements as it may think fit for the completion of supplies on account and at the risk of the suppliers (s). The additional expenses thus incurred together with the consequential losses and also the liquidated damages shall be recovered from the supplier out of his / their security deposit / earnest money deposit and any other amount due to him / them. The balance still, if any, payable by the supplier shall be paid by him/them within 7 days of notice by the Dr.Y.S.R Horticultural University

**FORFEITURE/REFUND OF THE EARNEST MONEY DEPOSIT(EMD)**

1. In case the selected Tenderer(s) does not supply the equipment at the quoted rates within the stipulated time and commits any breach of any one or more of these terms and conditions, the Earnest Money Deposit deposited by the Tenderers (s) will be forfeited.
2. Earnest Money of the unsuccessful Tenderer (s) shall be refunded within three months from the date of decision regarding the tenders. No interest is payable by the University on such deposit.
3. On due performance and satisfactory completion of the order in all respects during the contract periods, the Earnest Money Deposit (Security Deposit) will be refunded to the Bidder (s) without interest within a period of 3 months with effect from the date of receipt of a request to this effect from the Bidder.

#### SETTLEMENT OF DISPUTES

#### Any difference or dispute arising out of or in connection with this tender or acceptance thereof or the contract that may be entered in consequence thereof, shall be decided by arbitration. The Chairman of the committee for purchase of the equipment, Dr.Y.S.R Horticultural University or his nominee shall be the sole arbitrator and the arbitrator’s decision shall be final and binding on the parties. The Tenderer(s) will have no objection to such appointment on any ground whatsoever including that such nominee, in his official capacity dealt with this matter at any stage.

1. The parties hereby agree that in the event of any dispute no cause of action shall arise in their favor to approach any court unless they have restored to and exhausted the remedy of arbitration as envisaged above.
2. The parties also do hereby agree that the contract envisaged by these terms and conditions shall be deemed to have been entered into at Dr.Y.S.R.H.U, V R Gudem and the courts at Eluru, West Godavari District alone will have jurisdiction to try and legal proceedings which may arise out of this contract. Neither party shall file any proceedings in any other Court.

**TENDER FORM**

**(Should be included in Financial bid only)**

From: To

 The Associate Dean

 College of Horticulture-

 Anantharajupeta, Railway Kodur -516105

 Annamayya (Dist), Andhra Pradesh**.**

Ref: 1. Your tender Notice No: NIT NO. /Dr. Y.S.R.H.U/2025-26Dated...........

2.EMD – D.D. No. ...................Dated..........................for Rs............................

\*\*\*

I/We have read the contents of the terms and conditions mentioned in your tender schedule and its enclosures and agree to abide by the same.

I/We hereby offer to Supply and Installation of Equipment to College of Horticulture, Anantharajupeta, Railway Kodur prescribed in the schedule (or such portion thereof as you may specify on the acceptance of tender) at the price given below.

I/We agree to hold this offer open for a period of 3 months from the date of acceptance of tender and shall be bound by communication of acceptance dispatched within a period of 15 days from the date of accepting the tender of the bidder.

I/We have also examined the requisite specifications of the material to be supplied and my / our offer is to supply the required material in accordance with the requisite specifications.

I/We have carefully considered all terms and conditions in Annexure I, II (part -1/2) and III and particulars regarding settlement of disputes and we have signed the same in token of consciously accepting the same and do hereby state that we accept them without any reservations and accordingly I/We quote the rates inclusive of all taxes, duties, transportation, insurance etc., as below.

Name of the item/Unit Unit price

The articles will be ready for delivery within ..........................days from the date of receipt of supply orders.

 Yours faithfully, Proprietor

 (Signature and stamp of the Tenderers

State legal status, whether Prop. /

 Partner / Registered firm / Company etc.)

Encl: Samples enclosed

EMD-DD No.......................................dated............................for Rs...........................